Homing Tests at Sea for 22 –24 June 2004

1. Open MVC on multibeam vehicle and cut 12V wires to transducer cable

2. Acquire battery for Benthos transponsder (two in the fridge)

3. Assemble and seal transponder housing

4. Make an anchor for transponder

5. Test multibeam AUV in tank with transponder

6. Write code for single beacon homing on AUV

7. Test code for surveying in transponder

8. Make sure we are not stomping on someone else’s release code in the area

9. Deploy transponder at sea on 22 June and deploy AUV, if time permits

10. Deploy AUV at sea on 23 June

11. Deploy AUV at sea on 24 June

12. Leave transponder at sea (should last about a year)

13. Perhaps just hang a transponder from the side of the ship.

14. Attach acoustic modem transducer to Zephyr and set up ATM-885 deck box

