CTD_AUV Pre-Launch Checklist

· Visual Check of Capture Line and Pole

· Remove fairings, check foam packs

· Check Battery and Tailcone Comps

· Check the Dummy Plugs

· Listen for Bathy Pump Sound

· Verify LISST In/Out Tubing Is In Place

· Be sure Fairings and Rings are Secure

· Verify all Three Access Doors are Secure

· Turn Strobe On

· Remove PTT Magnet

· Dummy Off The Tether

· Remove CTDWetting Tubes

CTD_AUV Post-Recovery Checklist

· Start up “resetdw” on laptop

· Rinse Instruments, Install Wetting Tubes 

· Inspect Tailcone mechanical couplings

· Check Tailcone Compensation

· Check Sphere Pressure

· Turn Off USBL, Strobe

· Install PTT Magnet

· Clean LISST Windows 

· Place Batteries On Charge

· Upload Data
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