FAU Docking Payload Pressure Vessel Modifications
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Drill and counterbore a new 7/16” connector hole


- Install a MCBHRA8F 





Exchange the connector for the coil resolver with one of the MCBHRA8F connectors
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Install (2) Seacon FAWM8 F connectors in existing holes





Other – Not shown:


Modify Socket_left and Right – widen and deepen pocket, add 7/16”-20 threaded hole in top


Modify old cable pass-thru to accept plug – not shown


Fabricate (2) plugs





Install (2) new MCBH8M connectors








