Two Sensor Coils on the Docking Station and one Source coil on the Docking Payload.  The 2 sensor coils have a common ground wire allowing a 3 wire connection.
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