Battery Charge Procedure
	DOCK
	VEHICLE

	1. HV to dock ON
	

	2.  “ss” – set state to 
“docked-nocharge”
	

	
	3.  Vehicle ON

	
	4. “ss” – set state to
“docked-nocharge”

	5. “pc”  - set power out current to 
“50.00 50.00”
	

	
	6. “sv” – set FAU output voltage to
“35.00 10.00”  - 35V 10A

	7. “ss” – set state to 
“docked-charge”
	

	
	8. “ss” set state to
“docked-charge”

	
	9. qtalk to battery and issue “#c0bc” – charge battery

	
	10. send “#c0wf” to battery – turn off watchdog

	
	11. send “?????” to battery – monitor battery status

	
	12. “rs” – read status of FAU
Montor temperature

	13. “rs” read status of FAU

Monitor temperature
	

	
	14. When finished “#c0bd” to battery – set to discharge mode

	
	15. “sv” – set output voltage

“28.00 10.00” 

	
	16. “sv” – set output voltage

“20.00 10.00” – run vehicle off of battery

	
	17. “ss” – set state to

“docked-nocharge”

	18. “ss” – set state to 

“docked-nocharge”
	


