=====================================


  Lantronix DeviceInstaller for

  -----------------------------------

  Windows 98/98SE/ME/NT4 SP6a/2000/XP

  -----------------------------------

  Software Release Notes

  -----------------------------------


  Version 3.6

  March 30, 2004


  Copyright (c) 2003-2004, Lantronix


=======================================





This document describes the Lantronix DeviceInstaller for
Windows 98/NT software release.

This document is divided into the following sections:



o Description

o Requirements

o Installation

o Upgrade Instructions

o New Features

o Resolved Problems

o Known Problems

o Technical Support





Description
===========


    This utility provides users a single application, with a graphical 
    interface and utilizing Microsoft's .NET Framework, to access various
    configuration functions for Lantronix networking products. This makes it
    easy to perform initial setup, IP address assignment, firmware upgrades,
    and configuration changes.


Requirements

============



    The following items are required to run DeviceInstaller:



    1.  Windows 98/98SE/ME/NT4 SP6a/2000/XP.



    2.  Microsoft .NET Framework v1.1.



    3.  Microsoft Internet Explorer 5.1, or later.


    4.  30MB free hard drive space.
    Windows XP:

    The "Internet Connection Firewall" must be disabled, or else 
    UDP Port 30718 must be available.  Otherwise, you will not be 
    able to detect or communicate with any devices on the network.
    To configure, go to the Control Panel, go to Network Settings, 
    select the corresponding network adapter, choose Properties, and
    go to the Advanced tab.


Installation
============


    The DeviceInstaller is distributed in a single image as a self-extracting
    executable. It is included on the CD packaged with the device server.
    This utility can also be downloaded from the Lantronix website.

    1.	The application installation directory defaults to
        C:\Program Files\Lantronix\DeviceInstaller, unless another folder is 
        selected during the installation process. 
        
    2.  A shortcut to this application is created on the Start/Programs menu. 

    NOTE: The Microsoft .NET Framework 1.1 must be installed.  If
    for some reason you received this setup utility without the .NET
    Framework, you can download it at the following URL:
    
    http://www.microsoft.com/downloads/details.aspx?FamilyId=262D25E3-F589-4842-8157-034D1E7CF3A3&displaylang=en

Upgrade Instructions
====================


    1.  The installation of DeviceInstaller 3.6 will not uninstall
        DeviceInstaller 2.0.
        
    2.  Any installations performed over DeviceInstaller 3.6 and up
        will automatically uninstall the previous version before
        installing the new version.
        
    To uninstall the DeviceInstaller utility manually, follow these steps:

    1.  Select Settings->Control Panel from the taskbar Start menu.
    
    2.  Double click on the Add/Remove Programs icon.
    
    3.  Under the Install/Uninstall tab, select DeviceInstaller in the
        Software list and then click Add/Remove. Follow the prompts.
        (Note: DeviceInstaller was the default Program Folder specified in
        the installation process.)




New Features

============
 
    1.  Now supports all subnets.
    2.  New IP assignment wizard designed to detect and correct PC & Network configuration issues during the IP assignment.
    3.  Built in TCP/IP tutorial.
 




Resolved Problems

=================

    1.  Supports XSDRIN units.





Known Problems

==============



    1.  Multiple devices cannot be upgraded at the same time.

    2.  Location of Custom Web Pages cannot be specified on the devices that
        support this feature.

    3.  The Document tab on the Configure Device window is saved via
        the File->Save menu item.  However, all the devices and their
        info are also saved in this file.  When a new search is initiated,
        the document information will be gone.  The information can be
        retrieved via the File-Open menu item.  A future release will
        associated the document information with the  hardware address
        and saved in a separate file.

    4.  If a device is set with DHCP enabled and AutoIP disabled and
        there is no DHCP server on the network, DeviceInstaller will not be
        able to discover the device.

    5.  Firmware recoveries through the serial port of a WiPort device cause 
        the wireless driver in the WiPort to become corrupt.  However, the firmware 
        recovery will succeed.  The wireless driver must then be reloaded via a 
        hard wired connection.


Technical Support
=================


    If you have a question about the DeviceInstaller utility, first 
    look in the online Help file. When the program is running, press 
    the F1 key to automatically display Help, or select Contents in
    the Help pull-down menu. This Help file can also be accessed 
    via the shortcut on the Start/Program menu.

    If you cannot find an answer, please try our website at
    www.lantronix.com/support.  If you still cannot find an answer,
    please contact Lantronix technical support at
    1-800-422-7044 US or 1-949-453-7198.


Copyright (c) 2004, Lantronix. All rights reserved.
Windows, .NET and Internet Explorer are trademarks of Microsoft Corporation.
