Homing Requirements:
Assumptions:


Start with near-bottom dock


DVL gives altitude (to 20 cm)


Start with MARS depth (1100 meters)

Bearing + Range important

Homing range >> navigation error + dock watch circle
Assume worst case navigation error: 10’s of meters.

Therefore assume homing range: 100’s of meters.

Homing error (displacement & angular) sufficient to engage dock.

