14 March AUV docking meeting notes:
Rob presented data

Integral term needed on altitude following

Nose dropped 5 degrees when speed was slowed

Can’t control depth (alt.) and pitch at the same time


What tests need to be done?


Reduce depth control offset


Servo off altitude?


Compass calibration



Check with Crossbow,



Perform calibration check



Cross bow level?



Control tuning for 1 m/s

Add cross track control – provide heading, verses pure pursuit 

Where is the water track done? 1m below vehicle

USBL saturation – pool testable
Parosci driver issue – Rich has looked at it – Hans 
FAU weight and buoyancy
Roll alignment before antenna interferes
