Mission Log

17 APRIL 2006

Started vehicle on battery due to problems with tether.

Tether problems determined to be tether not plugged into Xantrex power supply and Ethernet cable not plugged in.

Ship power to Xantrex interrupted several times during transit.  Apparently problem with dedicated breaker tripping off line.

RF Ping running

Drop weight reset running

Battery cell volts min 4.09
TD newTailCone 
sat

TD crossbow
sat

TD parosci
sat

TD dvl
sat

TD gps
 -- received “bad hemisphere value” error message
fanTest – sat 17.7 % humidity, 81.9 F,
Launch at 0913
Mission 2006-107-01
Mission File c:\dorado\missions\CrossCal.cfg

Start at 0917
Dive at n/a
Surface NLT

Actual surface

Mission 2006-107-02

Mission File c:\dorado\missions\CrossCal.cfg

Start at 0919

Dive at n/a

Surface NLT

Actual surface

Mission 2006-107-03

Mission File c:\dorado\missions\CrossCal.cfg

Start at 0924

Dive at n/a

Surface NLT

Actual surface

Mission 2006-107-04

Mission File c:\dorado\missions\CrossCal.cfg

Start at 092X

Dive at n/a

Surface NLT

Actual surface

Mission 2006-107-05

Mission File c:\dorado\missions\CrossCal.cfg

Start at 0932

Dive at n/a

Surface NLT

Actual surface

Previous attempts all failed on kearfott.

Mission 2006-107-06
Mission File c:\dorado\missions\CrossCal.cfg

Start at 0935
Dive at n/a

Surface NLT

Actual surface

Mission 2006-107-08
Mission File c:\dorado\missions\CrossCal.cfg

Start at 0947
Dive at n/a

Surface NLT

Actual surface

Mission 2006-107-08
Mission File c:\dorado\missions\box500-10.cfg
Start at 1015
Dive at 1015
Surface NLT 1053 
Actual surface 1044
Lost rf comms. Drop weight server countdown initiated.

Recovered vehicle and placed on tether before drop weight lost.

Ended up resetting battery and turning off battery watchdog.  Believe issue was initial start of AUV was on battery instead of on power supply.  No explanation for long delay until failure.

Mission 2006-107-09
Mission File c:\dorado\missions\OutBack500.cfg
Start at 1158
Dive at 1158
Surface NLT 1218 
Actual surface 1211
Mission 2006-107-10

Mission File c:\dorado\missions\OutBack500.cfg

Start at 1220
Dive at 1221
Surface NLT  1238
Actual surface 1232 

Lost RF comms.  Recovered vehicle, reset stack with tether and launched.

Mission 2006-107-12

Mission File c:\dorado\missions\OutshoreDocking.cfg

Start at 1320

Dive at 1321

Surface NLT  1358

Actual surface 1331
Data showed CPA on transponder was > 100 meters.  Decided xpdr was too close to the bottom.  Raising to 3 meters above bottom.
Mission 2006-107-13

Mission File c:\dorado\missions\OutshoreDocking.cfg

Start at 1357

Dive at 1358

Surface NLT  1436

Actual surface 1410

Mission 2006-107-13

Mission File c:\dorado\missions\OutshoreDocking.cfg

Start at 1428

Dive at 1429

Surface NLT  1446

Actual surface 1442

Mission 2006-107-14
Mission File c:\dorado\missions\OutshoreDocking.cfg

Start at 1456
Dive at 1457
Surface NLT  1514
Actual surface 1509
Last mission is 15 not 14….
