Mission Log

21 June 2006

1244 Shanna Rae is anchored off MISO.  Vehicle is powered up on tether and comms are established via tether and RF.

Have window running resetdw, ping to RF and ping to tether.

Initial checks using TD 

TD new TailCone, sat

Td crossbow, with in a degree of ships heading from WinFrog

TD parosci, sat

TD dvl, sat.

TD gps, sat.

fanTest 64.9 cPa, 105.2F, 10.3 RH

Enabled battery

$B6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

1412 launch vehicle
1418 started mission 172.00
Mission file c:\dorado\missions\CrossCalDepth2.cfg

Mission end NLT 1424

Mission end 1420

TD bluefinBatt
$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

1433 run mission 172.01

Mission file c:\dorado\missions\CheckonSurf.cfg
Vehicle starts to circle.
SSS transmitted.

1437 run mission 172.02

Mission file c:\dorado\missions\CheckonSurf.cfg

SSS

1438 run mission 172.03

Mission file c:\dorado\missions\CheckonSurf.cfg

Unable to get vehicle to drive compass course away from kelp.  Recovered vehicle instead.  Decided that trim was nose heavy, removed 2 pounds of lead forward.  Estimated buoyancy is now 9 pounds.

Launched vehicle with safety tether, floated OK, released vehicle and resumed operations.

1544 run mission 172.0x
Mission file c:\dorado\missions\crosscal.cfg

Mission aborted on tailcone error?

1546 run mission 172.0x1

Mission file c:\dorado\missions\crosscal.cfg

Mission ended 1551
TD bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18
1557 run mission 172.0x2

Mission file c:\dorado\missions\crosscal.cfg

Mission aborted on parosci

1558 run mission 172.0x2

Mission file c:\dorado\missions\crosscal.cfg

1602 mission complete.  

1626 run mission 172.0x3
Mission file c:\dorado\missions\OutBack2.cfg
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