Mission Log

21 June 2006

1244 Shanna Rae is anchored off MISO.  Vehicle is powered up on tether and comms are established via tether and RF.

Have window running resetdw, ping to RF and ping to tether.

Initial checks using TD 

TD new TailCone, sat

Td crossbow, with in a degree of ships heading from WinFrog

TD parosci, sat

TD dvl, sat.

TD gps, sat.

fanTest 64.9 cPa, 105.2F, 10.3 RH

Enabled battery

$B6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

1412 launch vehicle
1418 started mission 172.00
Mission file c:\dorado\missions\CrossCalDepth2.cfg

Mission end NLT 1424

Mission end 1420

TD bluefinBatt
$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

1433 run mission 172.01

Mission file c:\dorado\missions\CheckonSurf.cfg
Vehicle starts to circle.
SSS transmitted.

1437 run mission 172.02

Mission file c:\dorado\missions\CheckonSurf.cfg

SSS

1438 run mission 172.03

Mission file c:\dorado\missions\CheckonSurf.cfg

Unable to get vehicle to drive compass course away from kelp.  Recovered vehicle instead.  Decided that trim was nose heavy, removed 2 pounds of lead forward.  Estimated buoyancy is now 9 pounds.

Launched vehicle with safety tether, floated OK, released vehicle and resumed operations.

1544 run mission 172.0x
Mission file c:\dorado\missions\crosscal.cfg

Mission aborted on tailcone error?

1546 run mission 172.0x1

Mission file c:\dorado\missions\crosscal.cfg

Mission ended 1551
TD bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18
1557 run mission 172.0x2

Mission file c:\dorado\missions\crosscal.cfg

Mission aborted on parosci

1558 run mission 172.0x2

Mission file c:\dorado\missions\crosscal.cfg

1602 mission complete.  

1626 run mission 172.0x3
Mission file c:\dorado\missions\OutBack2.cfg

Day 173

Td bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18

$b6q0 d- 32.01 2.06 19.92 3.97 4.01 0 -22936.26 00:45:28

1401 Run mission 173.00
Missions file C:\dorado\missions\CrossCal.cfg

1414 Run mission 173.01

Missions file C:\dorado\missions\Checkon5Meterdepth.cfg

1426

Td bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18

$b6q0 d- 31.89 2.13 19.23 3.95 3.99 0 -22993.55 01:13:51 m

Recovered vehicle and adjusted trim (again!) moved 4 pounds aft from Hydorscat to midpoint of battery section.  Visual inspection of tailcone assembly (strike on tailcone during last launch was worrisome) showed no damage.  Oil reservoir full, no indication of oil leak.
1529 launched again

1533 Run mission 173.02
Missions file C:\dorado\missions\TransitSet.cfg

1546
Td bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03

$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07

$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18

$b6q0 d- 31.89 2.13 19.23 3.95 3.99 0 -22993.55 01:13:51 m

$b6q0 d- 31.55 2.13 18.94 3.91 3.96 0 -23086.59 02:34:14 m

1601
Run mission TransitSet1000.cfg
Estimate 1614

NLT 1618

1619
Td bluefinBatt

$b6q0 d- 33.24 0.00 18.55 4.13 4.15 0 -22885.75 00:29:03 m
$b6q0 d- 32.93 2.02 18.55 4.10 4.12 0 -22921.00 02:04:07 m
$b6q0 d- 32.47 2.02 17.67 4.04 4.07 0 -23066.61 03:34:18 m
$b6q0 d- 31.89 2.13 19.23 3.95 3.99 0 -22993.55 01:13:51 m

$b6q0 d- 31.55 2.13 18.94 3.91 3.96 0 -23086.59 02:34:14 m

$b6q0 d- 31.39 2.13 18.65 3.88 3.93 0 -23176.59 03:07:30 m

1628
Run mission box500-8.cfg

Estimate 1645
NLT 1704

June 23, 2006
TD new TailCone, sat

Td crossbow, sat

TD parosci, sat

TD dvl, sat.

TD gps, sat.

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

0959 start c:\dorado\missions\CheckonSurf.cfg
Abort on tailcone

1001 restart

Abort on tailcone

1006 third start 

NLT 1014

Surfaced at 1011
1012 XMT SSS

Pull data.

Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m
Changed CheckonSurf.cfg to be depth controlled to 0 meters instead of pitch control to 0 meters. Changed heading to 350 from 330.
1022 start
End NLT 1030
1029 XMT SSS

Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m
1046 start TransitSet1.cfg
1047 start again TransitSet1.cfg

End NLT 1058

1054 Surface 

1056 XMT SSS

1100 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m
1100 Vehicle position 

3637.0728N 12152.5065W

1120 Run InshoreDock.cfg

1130 surface at GPS fix point, continued on.

1138 surface

1139 XMT sss

End NLT 1155

1147 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

1148 Vehicle position 

3636.5672n 12152.5199w
1204 Mission start
1216 Surface
1217 XMT SSS

End NLT 1223

1222 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

$b6q0 d- 30.58 2.35 16.99 3.79 3.83 0 -23043.91 03:55:35 m

1318 Start GoBack.cfg
1327 XMT SSS

END NLT 1328

1329 start InshoreDockLow.cfg
Aborted on resource unavailable

Soft reboot of vehicle

1331

1333 Start InshoreDockLow.cfg

1345 Surface
1346 XMT SSS

1350 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

$b6q0 d- 30.58 2.35 16.99 3.79 3.83 0 -23043.91 03:55:35 m

$b6q0 d- 30.32 2.35 17.48 3.76 3.80 0 -23223.34 05:24:44 m

1400 Start InshoreDockLow.cfg
1412 surface
1413 XMT SSS

NLT 1415

1418 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

$b6q0 d- 30.58 2.35 16.99 3.79 3.83 0 -23043.91 03:55:35 m

$b6q0 d- 30.32 2.35 17.48 3.76 3.80 0 -23223.34 05:24:44 m

$b6q0 d- 30.20 1.91 17.28 3.74 3.78 0 -23300.66 05:51:12 m
1430 Start InshoreDockLow.cfg

Still on surface but various mission processes are running.

1435 XMT SSS

1437 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

$b6q0 d- 30.58 2.35 16.99 3.79 3.83 0 -23043.91 03:55:35 m

$b6q0 d- 30.32 2.35 17.48 3.76 3.80 0 -23223.34 05:24:44 m

$b6q0 d- 30.20 2.31 18.06 3.74 3.78 0 -23333.16 06:11:04 m

1439 Start InshoreDockLow.cfg

1444 abort to surface

1444 XMT SSS

1447 Battery Status

$b6q0 d- 31.43 2.21 16.99 3.90 3.94 0 -22674.29 01:18:35 m 

$b6q0 d- 31.32 2.35 17.28 3.87 3.92 0 -22728.47 01:49:34 m

$b6q0 d- 31.16 2.28 17.48 3.85 3.91 0 -22768.72 02:10:04 m

$b6q0 d- 30.93 3.26 17.48 3.84 3.89 0 -22822.75 02:33:26 m

$b6q0 d- 30.70 2.02 17.28 3.81 3.85 0 -22951.60 03:20:59 m

$b6q0 d- 30.58 2.35 16.99 3.79 3.83 0 -23043.91 03:55:35 m

$b6q0 d- 30.32 2.35 17.48 3.76 3.80 0 -23223.34 05:24:44 m

$b6q0 d- 30.20 2.31 18.06 3.74 3.78 0 -23333.16 06:11:04 m

$b6q0 d- 30.12 2.35 18.06 3.73 3.78 0 -23354.49 06:20:58 m

Went to vehicle by small boat to check for drop weight.  No drop weight.
Recovered vehicle.

Voltage meter across drop weight leads gives 0.2 to 0.6 volts DC.

No more spare drop weights or burn wires available.  Done for the day.

