Mission Log

July 6, 2006

0730 Vehicle turned on, battery enabled, power supply held at 34.5 V to minimize discharge.

Have window running resetdw, ping to RF and telnet to RF.

TD newTailCone, tailcone wiggles, prop spins.
TD Crossbow heading matches ship heading.

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01
TD parosci, sat

TD dvl, sat.

TD gps, sat.

fanTest 61.3 kPa, 27.0/80.5 C/F, 9.5 RH

Physically verified presence of dropweight.

Launch 0835

0836 fanTest 62.2 kPa, 27.5/81.5 C/F, 9.8 RH

First mission is OffshoreHoming060706.cfg
0840 failed start, operator error in selecting directory

0844  Mission start
0846 Dive

Estimated 0903

End NLT 0906
Surface 0858
SSS 0859

Resetdw verified at 0900

0905 
fanTest 

62.2 kPa, 26.0/78.8 C/F 9.8 RH

62.2 kPa, 27.5/81.5 C/F, 9.8 RH

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01

$b6q0 d- 32.01 2.24 15.91 3.98 4.01 0 -19398.53 01:49:01
0921 
Run GoBackOffshore.cfg

Failed start, OE in td gps at the time

0923 restart GoBackOffshore.cfg

NLT 0928

0928 sss

0930 Mission Start OffshoreHoming060706.cfg
0931 dive on heading 220-230
NLT 0950 

Estimate 0947 

0942 surface
0944 sss

0944 watchdog is reseting.

1006

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01

$b6q0 d- 32.01 2.24 15.91 3.98 4.01 0 -19398.53 01:49:01

$b6q0 d- 31.66 2.28 16.21 3.93 3.97 0 -19533.59 02:45:34

1016 mission start InshoreBox060706.cfg
1017 dive on heading 240
Estimate 1028

NLT 1039

1029 surface
1030 sss

1030 watchdog is resetting

Down loading data

1034 running GoBackOffshore.cfg

1040 sss
1042

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01

$b6q0 d- 32.01 2.24 15.91 3.98 4.01 0 -19398.53 01:49:01

$b6q0 d- 31.66 2.28 16.21 3.93 3.97 0 -19533.59 02:45:34

$b6q0 d- 31.24 2.35 16.99 3.88 3.92 0 -19649.76 03:20:36
1043

fanTest 

62.2 kPa, 26.0/78.8 C/F 9.8 RH

62.2 kPa, 27.5/81.5 C/F, 9.8 RH

62.2 kPa, 26.5/79.6 C/F, 9.8 RH

1049 mission start InshoreBox060706.cfg  16
1050 dive on heading 240

Estimate +12 1101
NLT +23 1112
1101 surface

1102 sss

1102 watchdog is resetting

Sitting about 15 meters from kelp with kelp on the antenna.  Moved in to inspect, tailcone looked clear, decided to run GoBackOffshore.cfg to clear the kelp bed.

1104 bad start on GoBackOffshore.cfg
1105 running GoBackOffshore.cfg

1114 sss

1115 watchdog is resetting, data download in progress

1125

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01

$b6q0 d- 32.01 2.24 15.91 3.98 4.01 0 -19398.53 01:49:01

$b6q0 d- 31.66 2.28 16.21 3.93 3.97 0 -19533.59 02:45:34

$b6q0 d- 31.24 2.35 16.99 3.88 3.92 0 -19649.76 03:20:36

$b6q0 d- 30.97 2.93 16.69 3.84 3.89 0 -19783.84 04:04:51
1127

fanTest 

62.2 kPa, 26.0/78.8 C/F 9.8 RH

62.2 kPa, 27.5/81.5 C/F, 9.8 RH

62.2 kPa, 26.5/79.6 C/F, 9.8 RH

62.2 kPa, 26.4/79.6 C/F, 9.8 RH
1129 mission start InshoreBox060706.cfg  16

1130 dive on heading 240

Estimate +12 1141

NLT +23 1152

11?? surface

11?? sss

11?? watchdog is resetting

Vehicle failed to surface, LXT tracking system showed it to be dead in the water with range and bearing matching a kelp patch.  Shana Rae maneuvered in close and we manned the rails to do a visual search. AUV spotted from the from the crow’s nest.  Small boat arrived and we transferred Brett and Thomas with light line and recovery pole while Shana Rae anchored nearby.  Recovery, held upside down with head in the water. Snag the latch with the pole at full extension, pull to the surface, clear the prop, physically verify the drop weight is present.  Side tow back to the Shana Rae, tie off on a long line on the stern.

1320

Battery status

$b6q0 d- 32.86 0.03 19.23 4.09 4.10 0 -19292.57 00:04:44

$b6q0 d- 32.47 0.03 14.55 4.05 4.07 0 -19292.89 00:25:01

$b6q0 d- 32.01 2.24 15.91 3.98 4.01 0 -19398.53 01:49:01

$b6q0 d- 31.66 2.28 16.21 3.93 3.97 0 -19533.59 02:45:34

$b6q0 d- 31.24 2.35 16.99 3.88 3.92 0 -19649.76 03:20:36

$b6q0 d- 30.97 2.93 16.69 3.84 3.89 0 -19783.84 04:04:51

$b6q0 d- 30.51 2.35 16.69 3.79 3.83 0 -20039.01 05:58:21

1343 recovered AUV.  Placed on ship’s power.
1348 Initiated manual battery charge.

1348 8 amps at 35.0 volts.

$b6q0 c- 30.89 5.87 17.38 3.85 3.87 0 -20058.05 06:28:05 m
1440 8 amps at 35.4 volts

$b6q0 c- 31.28 5.61 21.48 3.89 3.91 0 -19908.32 07:18:08 m

1500 8 amps at 35.5 volts
$b6q0 c- 31.43 5.90 22.26 3.90 3.93 0 -19840.85 07:40:33 m

1503 5 amps at 33.9 volts

$b6q0 c- 31.32 3.26 22.36 3.88 3.91 0 -19836.20 07:42:28 m

1557 secured charge to shift to shore power.
1611 restarted charge

$b6q0 c- 31.43 3.00 21.97 3.89 3.93 0 -19761.28 08:49:27 m
1629
$b6q0 c- 31.55 2.93 22.75 3.91 3.94 0 -19735.41 09:07:40 m
1644

$b6q0 c- 31.62 3.00 23.43 3.91 3.94 0 -19712.92 09:22:54 m

