Mission Log

July 7, 2006

0645 Vehicle turned on.

Have window running resetdw, ping to RF and telnet to RF.

Enabled battery

TD newTailCone, tailcone wiggles, prop spins.

TD Crossbow is approximately in congruence with ships heading.

0722 Shifted to ships power from shore power.

0725 

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41

fanTest
61.3 kPa, 23.5/74.3 C/F, 10.0 RH

TD parosci, sat

TD dvl, sat.

TD gps, sat.

Physically verified presence of dropweight.

0755 Launch 

LXT is tracking

fanTest

61.3 kPa, 25.1/77.1 C/F 9.8 RH

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41

$b6q0 d- 31.39 2.50 14.55 3.90 3.94 0 -19782.50 00:58:45

0836 fanTest 62.2 kPa, 27.5/81.5 C/F, 9.8 RH

First mission is OffshoreHoming060706.cfg

0803 Mission start
0804 Dive

Estimate +12 0816
NLT +23 0826
???? surface

???? sss

???? watchdog is resetting

Brett in the water, recovery from kelp.  Verified dropweight installed. Cleared kelp from prop, it spins freely.

0835 GoBackOffshore.cfg
0843 sss

Resetdw is running

0854

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41 m
$b6q0 d- 31.39 2.50 14.55 3.90 3.94 0 -19782.50 00:58:45 m
$b6q0 d- 30.82 1.84 15.62 3.83 3.87 0 -19957.84 01:53:05 m

0910 Run CrossCal.cfg with -5 rudder on surface at speed 1.5.  Vehicle is porpoising more than desired.

Determined to run at slower speed and do a CW and CCW set of circles.  Rob set up new cal file CrossCal
0925 started CrossCal060707.cfg

EST +10 0935
NLT +11 0937

0940 completed cal, heading from crossbow seems to correlate with headings called by visual inspection.

0942

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41 m
$b6q0 d- 31.39 2.50 14.55 3.90 3.94 0 -19782.50 00:58:45 m
$b6q0 d- 30.82 1.84 15.62 3.83 3.87 0 -19957.84 01:53:05 m

$b6q0 d- 30.66 2.39 16.01 3.80 3.84 0 -20054.21 02:44:16 m

0955 +0 Mission start

0956 +1 Dive

Estimate +32 1028
NLT +37 1032
Surfaced momentarily at 1000 then dove.

Surfaced momentarily at 1012 
Surfaced at 1019

1019 surface

1026 sss

Dropweight server hung, manually reset, 

1029 watchdog is resetting

1053

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41 m
$b6q0 d- 31.39 2.50 14.55 3.90 3.94 0 -19782.50 00:58:45 m
$b6q0 d- 30.82 1.84 15.62 3.83 3.87 0 -19957.84 01:53:05 m

$b6q0 d- 30.66 2.39 16.01 3.80 3.84 0 -20054.21 02:44:16 m

$b6q0 d- 30.35 2.31 16.11 3.77 3.81 0 -20229.45 03:55:29 m
Mission CrossCalDepth.cfg

1058 +0 Mission start

1059 +1 Dive

Estimate +5 1103
NLT +7 1105
1106 surface

1108 sss

1108 watchdog is resetting

1112 GoBackOffshore.cfg

False start
1115 GoBackOffshore.cfg

Estimate +10 1125
NLT +10 1125
1124 GoBack.cfg
Estimate +3 1127
NLT +5 1129
InshoreBox060706.cfg

1151 +0 Mission start

1151 +1 Dive

Estimate +12 1203
NLT +23 11214
1204 surface

1205 sss

1207 watchdog is resetting

GoBackOffshore.cfg with speed at .8

1211 +0 Mission start

Estimate +5 1216
NLT +6 1217
1218 sss

1219 watchdog is resetting
1220

Battery Status

$b6q0 d- 31.58 0.03 14.16 3.93 3.96 0 -19765.25 00:26:41 m
$b6q0 d- 31.39 2.50 14.55 3.90 3.94 0 -19782.50 00:58:45 m
$b6q0 d- 30.82 1.84 15.62 3.83 3.87 0 -19957.84 01:53:05 m

$b6q0 d- 30.66 2.39 16.01 3.80 3.84 0 -20054.21 02:44:16 m

$b6q0 d- 30.35 2.31 16.11 3.77 3.81 0 -20229.45 03:55:29 m

$b6q0 d- 29.97 1.91 16.30 3.72 3.76 0 -20504.07 05:22:20 m
1225 +0 Mission start

Estimate +5 12306

NLT +5 1230
???? sss

???? watchdog is resetting

1228 +0 Mission start

1229 +1 Dive

Estimate +12 1240
NLT +23 0826

1239 surface

???? sss

???? watchdog is resetting

Vehicle recovered and griped down.
On tether with ships power, battery disabled.

**********************
???? +0 Mission start

???? +1 Dive

Estimate +12 0816

NLT +23 0826

???? surface

???? sss

???? watchdog is resetting

