Mission Log

July 31, 2006

0600

Trim and ballast in test tank.  Vehicle is 9 pounds buoyant.

0800 on Zephyr,

Checking in and modifying USBL driver code.

Vehicle is on tether and has good comms via tether and RF.

Resetdw is running.

Battery status is 

$b6q0 d- 33.44 0.00 20.80 4.15 4.17 0 -14140.91 00:05:08 m

fanTest
62.2 kPa 30.0/86.0 C/F 8.3 RH

0841 underway

TD newTailCone, tailcone wiggles, prop spins

TD crossbow, heading tracks with ships heading

TD dvl, chirps and tracks.

TD gps tracks ships location

1055
Launched vehicle.

1103

Initiatied compass cal using “Han’s Procedure”.  Noted that devices.cfg.cal does not exist but devices.cfg.compassCal does.  Used that instead.

Started crossCal060707.cfg

End NLT 1115
SSS 1113
1117 GoBack.cfg fail start

1118 GoBack.cfg

1123 sss

1124 box500-10-060707.cfg

1129 vehicle surfaced on abort
1129 GoBackOffshore.cfg

1135 GoBackOffshore.cfg

1151 box500-10-060707.cfg
1153 sss
1159 GoBackOffshore.cfg

1201 sss
1249 edited devices.cfg to remark out ctd

1254 running crossCal060707.cfg again

1309 running crossCal060707.cfg again after taking care of compassCal and normal cfg files also
1320 GoBackOffshore.cfg

1323 sss

1325 box500-10-060707.cfg

1357 sss
