AUV Docking Mission Log
13 March, 2006
6:30 Arrive, switch cradles with CTD vehicle, load on Zephyr

7:30 Adjust LARS, remove rail cross support

8:30 Depart Moss Landing

9:35 Arrive MISO; deploy transponder at waypoint 1, 325m N-NW of MISO

9:50 Launch AUV 

10:00 Run compass cal; .8 speed, ~10m circle open loop with compass in cal mode

– aborted early

10: 15 re-run compass cal

10:25 surface run for 5min at 300 deg; ran circle because compass was still shut down

10:30 re-run surface run; looks good; aborted early

10:40 start Rob’s offshore box: offshorebox.cfg
10:50 mission stopped because of syntax error, line 101 didn’t have a semicolon

10:55 repaired mission, copied over and re-started

11:05 mission ended as expected; tried to downloaded mission data; hadn’t ended mission so Rob’s download script didn’t work and it took 25 min to figure it out.

11:30  constructed new mission with 3 passes, downloaded and started offshortbox3x.cfg
11:45 mission stopped after one pass because the overall mission timer wasn’t modified for 3 passes

11:55 Re start 3-pass

12:43 3 pass ended

12:45 1km north, gps, 1km back mission started “outback.cfg”

12:55 transponder moved to inside box position, altitude changed to 5m off seafloor

1:10 1km out/back mission ended; ~125m SE of expected endpoint; downloading data

1:30 starting InshoreBox.cfg; failed to start
1:35 re-starting InshoreBox.cfg

1:50 on the surface

2:00 run altitude following mission 

2:20 on surface, downloading; new mission for low speed during homing speed=1 7as.cfg
2: 30 starting run

2:40 on surface; downloading new mission for low speed and 5m altitude

2:43 starting run 5as.cfg; parosci driver crashed again; restarting; on surface a long time
3:00 on surface; recovering AUV and transponder; 
3:15 heading for Moss Landing

4:25 on the dock

Pulling tail cone for CTD vehicle

