Docking AUV Trim and Ballast
Ballast and trim weights in pounds.

Locations are described in inches from nose of vehicle.

09MAR2006

Ballast

10 lbs in soft bag mounted to forward face of 10” bulkhead, below center axis.

Trim check showed level with base of antenna above water line.

Weights entered and calculated below.

[image: image1.emf]Test Weight, in air 12

Calculated Test Weight in water (x 0.9) 10.8

Weight shallow 4

Weight deep 5.5

Calculated Vehicle bouyancy with entrained air 6.8

Calculated Entrained Air 3

Calculated Vehicle bouyancy 3.8


