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Sample Container Design

VOLUME; 2.0 LITERS


OVERALL LENTH; < 20.5”


DIAMETER; AS REQUIRED*


FILL TIME: < 5 SECONDS


QUANITY IN STD MID BODY; 12


ENDS CAPS & PISTON*; UHMW PE


SAMPLER BODY*; PRECISION POLYCARBONATE TUBE


GUIDE ROD, VALVE, SPRINGS, FASTENERS; TITANIUM


SEALS; POLYURETHANE (POLYPAK)


PRESSURE COMPENSATION DIAPHRAGM; SILICON














