NODECONTROLLER_092806-1100 SPECIFICATION READ-ME
File Name:  NODECONTROLLER_092806-1100.MAX
QTY: 24 up array panel
Turn Time: 5 Days 

Layers: 4 

Layer Orientation:


1: TOP


2: GND


3: PWR

4: BOT

Thickness:  0.062 "" FR4 

Dimensions: 1" x 2" 

Plating: SMOBC 

Cu Weight: 1oz (TOP,BOT) 2oz (GND,PWR) 

Trace width/space: 0.007”/0.007”
Smallest hole size: 0.010" 

Sides to solder mask: Both Sides (BLACK)

Sides to silk screen:  Both Sides (WHITE) 

IPC-356 included for test! (NODECONTROLLER_092806-1100.net)
