Gulper Pressure chamber testing October 2007:
We fired four Gulpers at the bottom of the test tank. Two of the four samplers were set aside as standards. The other two gulpers were individually placed in a bag of DI water and cycled 10 times. The first was cycled to 375 psi (approx 250m), and the second was cycled to 150 psi (100 m). The sample cycled to 375 psi had approximately 39.5 ml of DI water in it, while the sample cycled to 150 psi had 7.6 ml of DI water in it. 

