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	Test diagonally across corner of test tank.  Magnetic coil in air.

All signals strong
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	Test along long axis of test tank. 

 Magnetic coil in air.

Source was shut off
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	Test along long axis of test tank. 

 Magnetic coil in air.

No magnetic or current signal with magnetometer at 1000 Hz, minimal at 100 Hz, 316 Hz OK

Magnetic signal & voltage signal strong at voltage sensor

Oddly, current at 100Hz appears weaker than current at 1000 Hz
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	Test along long axis of test tank.  

Magnetic coil in air.

Used zinc detectors for voltage measurement


