Control Room Console WAGO Fieldbus Configuration:

JOYSTICK Input:

Modules

Coupler = 750-341 Modbus TCP/IP Ethernet 


Device Name = wjoy


Domain = TIB.MBARI.ORG


IP Address = 134.89.21.21


Subnet Mask = 255.255.255.224


Gateway = 134.89.21.1

Digital input module = 750-430 (8ch, 24V input)


CH-1 = Joystick up


CH-2 = Joystick down


CH-3 thru 8 = N/C

Termination module = 750-600

Orange cable pin out: (5 pin mil connector)

A = N/C (GRN)

B = COMMON (BLU)

C = DOWN (GRY)

D = RIGHT (YEL)

E = UP (ORG)

