1. Work around 30k upload limit.

2. Remove Max. 2048 files limitation.  Ideally, this would be accomplished by a mechanism to remove files after they’ve been uploaded to next level.  Requires a CRC check or similar to ensure data integrity.

3. Batteries!  Does the SeaHorse power the CTD, and why does the CTD stop profiles when it’s internal batteries get low, even though the External supply remains high?

