BENTHIC ROVER DEPLOYMENT EQUIPMENT CHECKLIST
August 2006, Atlantis Cruise.

Tools:
· Oil Comp Filler/gauge



x
· Screwdrivers





x
· Wrenches





x
· Socket Sets





x
· Hex drivers





x
· Cordless Drill
· Drill set, up to ½”

· Burr-tool





x
· Pliers






x




· Vise-grip

· Diagonal cutter




x
· Hacksaw

· Files

· 1/4-20 tap and die
· 3/8-16 tap and die
· Utility knife

· Tape measure





x
· Caliper

· Dummy burn wires




x

· Multi-meter

Expendables:

· Aqua Lube (2)





x
· Silicon Spay lube, food grade (2)


x
· O-ring Lube, Dow #55 (2)



x
· Tape, electrical (4)




x
· Teflon Tape, ½” wide
(2)



x
· Tellus 15 Oil, 5 gal. w/ MSDS


x
· Zip Ties, various sizes




x
· Rope, ¾” Yellow Poly, 60ft



x
· Rope, ¼” Spectra or Nylon, kernmantle, 80ft

x
· Air-can duster
(2)




x
· Batteries (C)

· Rover dunnage




x
Spares:
· Ti Fasteners, assorted




x
· Stainless fasteners, assorted



x
· Clamp-brackets




x
· Comp hose





(ordered)
· Comp Hose fittings





· General SS Hose Clamps



x
· Large SS Hose Clamps



x
· Ti Hose Clamps




(ordered)

· Ti welding rod (bearing lock pins)


x
· HDG shackle (line to spar buoy)


x
· O-rings

· Drive belts (1)





x
· Bearings





x
· Drive pulleys (2)




x
· Spar pole (1)
· RF Beacon (VHF 73) 




x
Deployment Hardware:

· Rover (1)





x

· Spar Buoy (1)





x
· Spar/Lift line





x

· Strobe (1)





x
· RF Beacon (Ch. B, 159.480 Mhz)


x
· Drop weight jack




x
· Drop weights (5)




x
· Drop weight eye bolts w/ 3 nuts (6)


x
· Drop weight release slings (6)


x
· Drop weight safety strap/carabineer


x
· Burn wires (6)

