Benthic Rover Highlights:
1. Benthic Rover chassis, propulsion system and floatation were designed and assembled at Scripps and delivered to MBARI in February 2006.

2. 6000m rated Ti housings for electronics, motor amplifiers, and batteries have been fabricated. The electronics wiring harness for the prototype Rover was fabricated and tested.

3. Software has been written to switch power to instruments, communicate with the current meter, and the motor drives.

4. Validated cable pack design during ROV sea trials. 

5. Designed drop weights, mounts, motor controller housings.
