Benthic Rover Connectors:

Red indicates not needed in 2006

Bulk head connectors:
1. From Seacon: (All Titanium)
a. MINM 25 -FCR, qnty. 2 (Scanners)

b. MINM 26 –FCR, qnty. 2 (Racks)
c. MINK 10 –FCR/L, qnty. 3 (Drive motors, Current meter, Camera/Light)

d. MINM12 –FCR/L, qnty. 2 (ROV/MARS, Batteries)

e. MINK 10 –FCR, qnty. 4 (guest instruments)

Total: 
13 (6)
2. From Subconn:

a. MCBH4F, qnty. 6 (Rack, Motors, Optode)

b. MCBH4F, qnty. 6 (Scanner Motors)

c. MCBH2F, qnty. 2 (Stir motors)

d. MCBH3F, qnty. 2 (Chamber cameras)

e. MCBH6F, qnty. 4 (Fluorometers, Ultrasound)

f. Total: 20 (10)
Cable connectors:
1. From Seacon: (all Titanium) could you also get a quote for molding cables to the CCPs (we will provide the cable)
a. MINM 25 –CCP, qnty. 2

b. MINM 26 –CCP, qnty. 2

c. MINK 10 –CCP/L, qnty. 3
d. MINM12 –FCR/L, qnty. 2 

e. MINK 10 -CCP, qnty. 4

Total: 13 (6)
2. From Subconn: 
a. MCOM4M, qnty. 10 (motors) (only need 4 now-BR purge, rack motors)
b. MCIL6M, qnty. 4 (with standard 24” unterminated whips) (fluorometer)
c. MCIL3M, qnty. 2 (with standard 24” unterminated whips) (Chamber cameras)
d. MCIL3F, qnty. 2 (with standard 24” unterminated whips) (Chamber cameras)

e. MCIL4M, qnty.2 (with standard 24” unterminated whips) (Optode)

f. MCIL4F, qnty.2 (with standard 24” unterminated whips) (Optode)

g. MCOM2M, qnty. 4 (BR stir and clean mtrs)

h. Total: 26 (10)
i. Could you also estimate how much an addition 12” of whip would be for the MCILxMs
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