Rover deployment plans 2007- winter 2008

May 21-29, 2007
8 day Rover deployment at Smooth Ridge, 1000m

This is an engineering test dive during which the Rover will visit up to 6 sites, each 10 m from the previous site. At each site the Rover will conduct respirometry experiments. Respirometery measurements are achieved by inserting a small cylindrical chamber into the sediment and measuring the change in oxygen saturation over time. We will use ROV observation on May 21 to monitor the Rover’s operation. The 250 lb drop weight will be recovered by an ROV.
Aug 27-Sep10, 2007
14 day Rover deployment at Smooth Ridge, 1000m

This is an engineering test dive during which the Rover will visit up to 12 sites, each 10 m from the previous site. At each site the Rover will conduct respirometry experiments. We will use ROV observation on Aug 27 to monitor the Rover’s operation. The drop weight will be recovered by an ROV.

Nov 7- Nov26, 2007
21 day Rover deployment at Smooth Ridge, 1000m
During this deployment Rover will visit up to 18 sites, each 10 m from the previous site. At each site the Rover will conduct respirometry experiments. We will use ROV observation on Nov 7 to monitor the Rover’s operation. The drop weight will be recovered by an ROV.

early Jan 2008


Short Rover deployment to test any features added to enable the Rover to plug into MARS

Winter-Spring 2008 Rover will be deployed on MARS

