Pt. Lobos/Ventana Deployment of Prototype Rover

Fri, July 7th
1) Mobilize Rover on ship

Mon, July 10th
1) Transit to 100 m water depth

2) Launch Rover over rail, freefall to bottom

3) Launch ROV

4) Observe Rover operation on bottom for ~1/2 hour

5) Acoustically release Rover drop weight, observe ascent

6) If acoustic release is not successful, pull release lanyard with ROV

7) Recover drop weight with ROV

8) Recover ROV

9) Recover Rover

Tue, July 11th
1) Transit to MARS node site at 1000 m water depth

2) Repeat dive sequence from Monday

Rover Weight is ~2000 lbs dry, ~150 lbs wet

Drop Weight is 240 lbs wet

