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Pre-deployment:

1. Install Rover battery shorting plug and deck comms cable.

2. Establish reliable comms with Rover through deck comms cable.

3. Check that relay board and motor controllers are on line. Do not attempt to turn the treads.

4. Power on the Acoustic Modem and wait for it to chirp. If no chirp is heard after ten seconds, cycle the power until the chirp is heard.

5. Verify that there is no voltage on the burn-wire leads.

6. Reattach burn wire connectors to release mechanism.

7. Check all flotation mechanically secure.

8. Check and record propulsion motor comp oil level.

9. Check that drop weight is installed properly and free to drop.

10. Remove drop weight safety strap.

11. Issue software command to start Rover programmed behavior, noting the exact time.

12. Unplug Rover deck comms cable and install dummy plug in its place.

13. Check all cable connectors and dummies installed and tight.

14. Check for tools left on and in Rover frame.

15. Remove “head banger” cushions from Rover Ti tubes.

16. Note Rover HomerPro channel number.

17. Activate Strobe and VHF Beacon on Spar Buoy, noting Beacon channel number.

18. Remove Rover hold-down straps.

Deployment:

19. Deploy Rover and Spar Buoy, noting exact time of launch.

20. Deploy topside Acoustic Modem Transducer from ship.

21. Establish comms between Rover and ship with Acoustic Modem.

22. Track Rover descent with HomerPro Ranger system on ship and note estimated time of landing.

23. Locate Rover with ROV.

24. Check Rover comp oil level at depth.

25. Observe Rover treads and their depth of penetration into the sediment.

26. Observe Rover programmed movement until last move is complete.

27. Deploy HomerPro on float near Rover, and then back ROV away at least 25 meters.

28. Establish comms with Rover Acoustic Modem.

29. Acoustically command a Drop Weight release, and observe weight drop and Rover ascent.

30. If Rover doesn’t ascend, rock Rover with ROV manip in case of mud stiction.

31. If Rover still doesn’t ascend, pull Drop Weight manual release lanyard.

32. Recover HomerPro with ROV manip.

33. Recover Drop Weight with ROV manip.

34. Recover topside Acoustic Modem Transducer.

35. Recover ROV.

Recovery:

36. Locate Rover on surface.

37. Recover Spar Buoy.

38. Attach Rover lift line to ship’s crane.

39. Recover Rover, noting exact time Rover is on deck.

40. Secure Rover with hold-down straps.

41. Turn off Acoustic Modem.

42. Turn off Spar Buoy Strobe and VHF Beacon.

