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Dive Objective: Test new control software, second attempt at first multi-incubation deployment, test transit camera and strobe.

Deployment Date: ___________

Recovery Date: ___________

Person performing topside checklist: 
_____________

Pre-deployment:

1. Install Rover battery shorting plug and deck comms cable.

2. Establish reliable comms with Rover through deck comms cable.

3. Run syntax check on mission code.

4. Run predive test program and verify correct operation of the following systems:

a. Valve Pumps run

b. Current Meter returns data

c. Rack motors lower chambers, limit switches stop motors, and racks return home

d. Propulsion Motor controllers communicate

e. Relay boards activate all relays

f. Stir Motors rotate

g. Optodes return data

h. Cleaning Pumps run

i. Chamber Cameras return images

j. Transit Camera returns images

5. Prime Valve Pump hosing with water on both stbd and port.

6. Power on the Acoustic Modem and wait for it to chirp. If no chirp is heard after ten seconds, cycle the power until the chirp is heard.

7. Check all flotation mechanically secure.

8. Check and record propulsion motor and rack comp oil levels.

a. Port propulsion comp level:
_____________

b. Stbd propulsion comp level:
_____________

c. Port rack comp level:
_____________

d. Stbd rack comp level:
_____________

9. Inspect all comp oil hoses and fitting for damage and leaks.

10. Check that Drop Weight is installed properly and free to drop.

11. Remove Drop Weight safety bars.

12. Activate Argos beacon on Rover, verifying operation with Cat’s Meow.

13. Activate Strobe and VHF Beacon on Spar Buoy, noting Beacon channel number.

a. Beacon channel number: ___________

14. Note HomerPro channel number.

a. HomerPro channel number: ___________

b. Rover start time:
_____________ PDT

15. Unplug Rover deck comms cable and install dummy plug in its place.

16. Check all cable connectors and dummies installed and tight.

17. Check for tools left on and in Rover frame.

18. Remove Rover hold-down straps.

Deployment:

19. Deploy Rover and Spar Buoy, noting exact time of launch.

a. Rover launch time:
____________ PDT

20. Deploy topside Acoustic Modem Transducer from ship after notifying bridge.

21. Establish comms between Rover and ship with Acoustic Modem and track Rover descent to at least 500m.

22. Track Rover descent with HomerPro and note estimated time of landing.

a. Rover landing time:
____________ PDT

23. Raise topside Acoustic Modem Transducer to safe depth, and then notify bridge.

On Bottom:

24. Check Rover comp levels on bottom with ROV cameras.

a. Port propulsion comp level:
_____________

b. Stbd propulsion comp level:
_____________

c. Port rack comp level:
_____________ 

d. Stbd rack comp level:
_____________

25. Record depth and location of Rover

a. Depth: _____________m

b. Latitude: _____________deg

c. Longitude: _____________deg

26. Estimate speed and direction of bottom currents as seen by ROV

a. Current speed:
_____________cm/sec

b. Current direction: ___________magnetic

27. Observe

a. Launch phase (no activity for 100 min from launch)

b. Rover moving 3.3 m to new site, taking 3 transit images

c. Rover waiting for sediment to settle (5 min)

d. Camera Light activation during frame capture (~30 sec)

e. Valves opening (~15 sec)

f. Chamber insertion and Sediment Switch activation (~1 min)

g. Valves closing (~5 sec)

h. Camera Light activation during frame capture (~30 sec)

i. Stir Motor rotation and optode reading (~1 min)

j. Valve opening (~15 sec)

k. Chamber cleaning and removal (~1 min)

l. Returning to step ‘b’ for a total of 2 cycles, then repeating a 3rd time but now turning to mission heading

m. Rover beginning long measurement cycle

28. Acoustic Modem comms

a. Lower topside Acoustic Modem Transducer to working depth after notifying bridge.

b. Open terminal session on laptop and capture to a file.

c. Establish comms between Rover and ship with Acoustic Modem.

d. Get Rover status with BR$STATUS.

e. If time permits, and the mission is still running, issue BR$ABORT command.

f. When ready to recover Rover, issue burn wire command, ‘AT$N0,107’, noting exact time

i. Burn wire command issued: ___________ PDT

g. Observe Rover drop weight release, noting exact time

i. Drop weight released:
___________ PDT

Recovery:

29. Locate Rover on surface, noting exact time.

a. Surface time: ___________ PDT

30. Recover Spar Buoy.

31. Attach Rover lift line to ship’s crane.

32. Recover Rover, noting time Rover is on deck.

a. Recovery time:
____________ PDT

33. Secure Rover with hold-down straps. 

34. Turn off Spar Buoy Strobe and VHF Beacon.

35. Turn off Acoustic Modem.

36. Turn off Argos Beacon.

37. Connect deck comms cable and retrieve mission data. 

38. Remove Rover battery shorting plug to disconnect battery and install dummy plug.

39. Remove deck comms cable and install dummy plug.

