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Pre-deployment:

1. Check all cable connectors and dummies installed and tight.

2. Establish reliable comms with Rover through AUV deck cable.

3. Turn port and stbd treads in both forward and reverse.

4. Acoustically command a drop weight release in air, and observe voltage on the burn-wire leads.

5. Cycle the power on the Acoustic Modem to cancel the burn.

6. Verify that there is no voltage on the burn-wire leads.

7. Reattach burn wire connectors to release mechanism.

8. Check that drop weight is installed properly and free to drop, but attached to Rover by a 2 ft keeper lead.

9. Check all flotation mechanically sound.

10. Check for tools left on and in Rover frame.

11. Lift Rover with crane just enough to take weight off of dolly wheels, then remove dolly wheels.

12. Deploy Rover.

Deployment:

13. Drive Rover to center of Test Tank, or as far as tether will allow. Run port and stbd treads in both directions.

14. Acoustically command a drop weight release, and observe weight drop and Rover ascent to end of 2 ft keeper lead.

Recovery:

15. Lift Rover out of tank and over deck, stopping at height of about 1 ft and when drop weight is touching deck.

16. Reattach dolly wheels.

17. Position Rover relative to drop weight so Rover can be lowered freely.

18. Lower Rover to put weight on dolly wheels.

19. Turn off Acoustic Modem

