Rover program outline for dive #6

Movement

1. Wakeup after timed delay

2. Observe current for 15 minutes and calculate current vector

3. Turn into current

4. Move up current 10 meters at V=1000

Measurement

5. Capture image of sediment

6. Lower chamber

7. Wait 30 seconds

8. Capture image of lowered chamber

9. Raise chamber to home position

10. Go back to #1, repeat for a total of three cycles

Final test

11. Execute a programmed square path 5 meters on a side, aligned with N, S, E, W

