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Benthic Rover Operation Outline for February ’07 Missions at M2
1. Launch Phase

· Sleep for X minutes – determined by ocean depth and ROV transit time

· Flash camera lights every couple minutes for 15 minutes for reassurance

2. Movement Phase

· Drive 10 meters away from current location, turning into current before moving forward

· Rover will not attempt to correct trajectory during forward motion
3. Measurement Phase

· Take image of sediment

· Open chamber valve

· Insert chamber into sediment

· Take image of chamber in sediment

· Close chamber valve

· Begin stirring action

· Record optode readings every 5 seconds for 1 minute, wait 14 minutes and repeat N times
· Stop stirring action

· Open chamber valve

· Move rack to home position

4. Acoustic Commands
· Run Mission with long/short measurement times

i. Long measure – execute optode recording 144 times (36 hours)

ii. Short (test) measure – execute optode recording 1 time
· Current status

· Abort current mission


