Function requirements for the interface to devices external to the electronics housing

1. Isolated power (or isolatable)

2. Current and voltage monitoring

3. Ground fault detection to 1 mA, min. detection from uAs to 1 mA

4. Fuses

5. Isolatable comms

6. No control lines (check instruments)

