Power Requirement

External components:

Groups:

Motors:

1. Scan 1 motors (3) +fluorometer

a. Power requirements:

i. 12-28 v, ~1.5 A for 3 motors

ii. 7-12 v, 100 mA motor logic (based on PIC Servo)

iii. 7-15 v, 80mA for fluorometer

2. Scan 2 motors (3) + fluorometer

i. 12-28 v, ~1.5 A for 3 motors

ii. 7-12 v, 100 mA motor logic (based on PIC Servo)

iii. 7-15 v, 80mA for fluorometer

3. BR1 purge and cleaning motors (2)

i. 12 - 24 v, >500mA (complete guess) for both

4. BR1 stirrer motor

5. BR2 purge and cleaning motors (2)

6. BR2 stirrer motor

7. Propulsion motors (2)

8. Rack 1 motor

i. 24v, 1A

9. Rack 2 motor

i. 24v, 1A

Core Instruments:

1. Current meter

2. BR1 camera

3. BR2 camera

4. Transit camera

5. Guest instruments (4)

6. Acoustic modems (2)

7. Optrodes (2)

