5V LOGIC

5V LOGIC

5V LOGIC 5V LOGIC

12V POWER

A ROVFLOW

ROVER SIGNAL FLOW DIAGRAM

4- 21- 93 ROVFLOW.S01 1 1 RCG

12V POWER RS- 232

Y/ C VIDEO, 12V POWER

12V POWER LOGIC

12V POWER

12V POWER

12V POWER

Y/ C VIDEO, 12V POWER

BURNWIRE

12 POWER

12V POWER, RS- 232

RELEASE- 2

ACOUSTIC TRANSMITTER

ARGOS

28 VOLT, TRIGGER SIGNAL

ANALOG

12 VOLTS

RS- 232

BOTTLE

NISKIN

STBD FOOTPAD

FOOTPAD

PORT

CONTROLLER

MICROPROFILER

PORT DRIVE MOTOR MOTOR

STBD DRIVE

STBD VIDEO CAMERA

STBD FLOOD LIGHT

BATTERY PACK- 2

BATTERY PACK- 1

CAMERA

PORT VIDEO

LIGHT

PORT FLOOD

(COMPASS, TILT- SENSOR, VIDEO CAMCORDERS)

CENTRAL CONTROLLER

ACOUSTIC RELEASE- 1

ACOUSTIC TRANSPONDER

TIME- LAPSE CAMERA

CAMERA STROBE

VANE

CURRENT METER

CURRENT METER ROTOR

ARM MOTOR

CURRENT METER

SENSOR SENSOR

STBD BENTHIC CHAMBER CONTROLLER

PORT FLOW PUMP

FLOW CELL

PORT

PORT STIR MOTOR

PORT PURGE VALVE MOTOR

PORT SLIDE VALVE MOTOR

PORT FLOW PUMP

FLOW CELL

PORT

PORT STIR MOTOR

PORT PURGE VALVE MOTOR

PORT SLIDE VALVE MOTOR

PORT BENTHIC CHAMBER CONTROLLER

PORT LEAD SCREW STBD LEAD SCREW

LIMIT- DOWN SWITCH

ASSEMBLY

INSTRUMENT LIMIT- UP SWITCH

ASSEMBLY

INSTRUMENT INSTRUMENT ASSEMBLY MOTOR

SENSOR

ODOMETER UP- SENSOR

ASSEMBLY

INSTRUMENT

A B C D

4

3

2

1

D C B A

1

2

3

4 Scripps Institution of Oceanography Dr. Ken Smith Laboratory

B Filename

Date

Title Rev

Drawn by Sheet of

Number

Size