Stan,

I need a penetrator good to 10,000 PSI that can bring two 1 mm acrylic optical fibers into an aluminum pressure housing.  I think a penetrator like your PNA-3/8 or PNA-1/2 in aluminum would work well for me.  The fiber cable I am experimenting with now has a black polyethylene jacket.  If the jacket cannot be bonded to, or you think there will be leaks, I can easily switch to an unjacketed cable if necessary (I will supply the fiber optic cable).  Please quote me for two of these assemblies.
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Thanks, Rob Glatts

Tel: 858-534-4858 x3

Fax: 858-534-7313

E-mail: rglatts@ucsd.edu
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