Scanner Lander Deployment June 18, 2001

Pulse Station 3714

The scanner lander was deployed in the Santa Catalina basin in 1300m water depth for about five hours.  The instrument ran through the program completely with only the scanner system failing.  Analysis of the video tape showed the scanner transducer unable to locate the sediment surface since it was apparently too soft.  The landing portion of the video showed the lander pistons nearly disappearing into the sediment upon hitting bottom.

The video shows the grab tray working properly with the grab and planar optode pushing into the sediment without disturbance.  All burnwires functioned properly with the grab valve and doors closed upon recovery.  The Niskin bottle had water in it upon recovery also.

