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PIN CONFIGURATION
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Receptacle Description

CAN H CANbus line (dominant high)
NCG Node Communication Ground
NCR Node Communication Request
Gnd Ground

Positive supply 5-14V positive supply

NCE Node Communication Enable
BOOT EN Boot Load Enable (do not connect)
CAN L CANbus line (dominant low)
RS232 RXD RS232 Receive line

RS232 TXD RS232 Transmit line
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