To update the firmware:
***********************
1.     Disconnect everything from the PSU. Connect a wire between SDA (CN7-4) and Th (CN7-3) to ground (CN7-2) to put the power supply in firmware upgrade mode.
2.     Apply main power..
3.     Start SCU 3.0.15 utility on host.
4.     Select FILE-OPEN from menu and select the firmware file.
5.     Select INIT-SETUP and select the following:
a.     Access Type: Select correct port type and address.
b.    Protocol: Select “Bus Timer and No Checksum”.
c.     Firmware Type: Select “HESC-UPS8”.
6.     Press OK button after HESC-SERD is initialized.
7.     Select INIT-FW UPDATE and press the START/STOP UPDATE button.
8.     Read the info from the dialog box and then wait 7-8 seconds , then press OK button.
9.     Remove the wires from CN7 'AFTER' firmware update is started.
10.  Close SCU after update is done.
11.  Remove main power.
12.  Wait for 30 seconds after power down.
13.  Apply main power again.
Note :  Once you put the Jumper and apply power do not attempt to disconnect the power in less than 10 seconds, otherwise  the PSU will not be able to recover the Firmware. 
