1/2/07, 1/31/07

Only Starboard side chamber optode and ref optode. Ref optode has always been S/N 799. Starboard chamber optode S/N 800 drifted on both Jan dives. It was sent to Aanderaa. We put optode S/N 801 on the starboard chamber. Aanderaa replaced S/N 800 with S/N 850. S/N 850(not positive about the number?) failed completely (no comms) during tank testing and was also sent back. We ended using S/N ? on the port side, which was taken off of Ken Smith’s current meter for May/June 07 and it was drifting too. We conducted tests on the ROV…

8/30/07

Moved optode S/N 799 (formerly the ref optode) into the port side chamber for dives on 9/10/07 (lobos) and 9/20/07 (flyer cruise). Waiting for a replacement from aanderaa for optode S/N 850, pulled off optode S/N 260 which drifted at depth.

9/21/07

optodes S/N799 (Port side),S/N 801 (Starboard Side) and replacement from Aanderaa S/N 485(ref) all worked although S/N 485 seemed noisy and our Starboard side valves were not working so the slope of the curve was unusual. 

