Benthic Rover Project Meeting 

10Apr08
Attending: Rich Henthorn, Brett Hobson, Paul McGill, Alana Sherman, Ken Smith
1) Project management

a. Move July ship date- Aug 1 is open but NO mob day…we also have Aug 18, could use one of the PC days Aug 5, 6

b. What to do with ship dates in light of mars- plan another autonomous deployment to test addition of fluorometry system, maybe go to Soquel canyon. Test cleaners
c. Roll over- waiting for Pinto to return (2/25) to fix missing $10k issue- Mike says ‘don’t worry we will fix it’
2) Next deployment April 15 – May 13
a. New features

i. Transit Camera and strobe

ii. Add third video camera to back of vehicle – not this dive
iii. Nice to have- load controller switching extra camera

b. Feature freeze on March 25

c. Correct control system

d. Battery test in tank for extended period (2-3 weeks)
i. Test tank booked March 31-April 11

ii. Need sturdy extenders for sediment switches

iii. Trigger artificial faults to test recovery

3) To Do list:
a. Software

i. Data stream for Rover – proposal has gone through one revision and the latest version looks good, will try out some initial config for this dive. Made changes to data stream format.
ii. Need to review current meter record to see if we should have seen a strong enough current – it appears that the current was not strong enough to exceed the threshold set in the algorithm. 
iii. Look into sleep mode with UPS- it works! We still need to find out more about recharging the batteries, is it smart enough to stop charging? It will sleep during an elapsed period of time. Why does it use so much power in sleep mode? Should be uAmps not mAmps, waiting for call from Technologic.
iv. Test external wake up from modem (Alana needs to wire it up)
v. Rich compiled list of errors only motor controller errors seem likely to kill mission
vi. Figure out how to turn the Ethernet back on

vii. Test Prosilicas custom driver for our stack – it works, Rich captured a still image.
viii. Add optode logging during descent and during insertion – 50% progress
ix. Can we add a safe mode to the code- don’t continue the mission because battery voltage is low or any other dangerous condition
x. Load Controller (Brian)

xi.  “Friendlier” method for starting missions (for Smith Lab techs)

xii. Need interactive interface for driving around MARS node

b. Mechanical:

i. Strobe chassis- Mount reflector and red light on circuit board

ii. Need to mount light and cameras
iii. Look into finding blue light (Brett), what voltage is the deep sea light

iv. New sphere is here but not yet machined

v. We need to make at least one more drop weight by next October

vi. Install new modem

vii. Mars extension cable pack, Brett will check with Larry about adding a test pack for next dive
viii. Cleaner –Brett is still thinking about it
c. Electrical

i. Strobe chassis (Brett)

ii. Sphere rewiring

1. Ethernet board
2. Relay switchers
iii. Test cable for strobes

iv. Check electrical connections to new camera and strobe
1. Need to test strobe with wet cabling
2. Need to determine how much current the strobes draw when charging

v. Battery pack needs to be changed
vi. Check on old camera cables for 3rd video camera- postpone until summer

vii. Check if there is a modem output that can be used to wake up the UPS

viii. Measure energy required for 1 mission- Paul will estimate based on spreadsheet calcs – TBD

ix. Paul got a blue light from Z, long pass filter (635 nm long pass filter) from Edmund are here (Paul) he built a mount for the filter. First impression is going to take a lot of light.
x. Optode data looks weird Alana- will look at data during the descent, done- data from descent is pretty inconclusive because there are still offsets but they are not even consistent with what we have been seeing. Alana needs to check the optode on Ventana during the Nov7 dive to see if it is reading similar values to those we collected.

d. Other:

i. Fluorescence imagining: 

1. Need to get Danelle up and running on fluorescent imaging, hopefully we can set up a test in the lab

2. Alana choose clips to be digitized (ProjectLibrary\900502.BenthicRover\Rover.Images\Rover.Video)

3. Paul will average the images and remove blue channel

ii. Tank testing:

1. Set reasonable current limits (for racks)
2. Run the respirometer in some sort of closed environment during testing
4) To Do for MARS deployment

a. Install low-power electronics so allow us to work on low-power modes

b. Remove spar buoy, replace with recovery line

c. Re-ballast new configuration

d. Practice moving the Rover

5) 2008 Ship time

a. Request change May 30 to Aug 5-6 – Granted

b. Request change June 17-18 to sometime Sept or later – Best available dates right now are Nov 4-5
