Rover Meeting October 16, 2008
1. Mechanical 

a. Port side valve was stuck because the o-ring extruded during priming.

i. Look into smaller o-ring or lessen the valves travel with spacer

ii. Write up procedures

b. Starboard middle valve stuck because spring was bound on urethane valve seat

i. Johnny will trim the valve seats down or make the new springs out of Ti

c. We will cold test all valves before next dive

d. Lift line wrapped around foam pack during deployment

i. The quick-release stuck and the float was deployed too early

ii. Next time we will not release the float until the rover starts to sink

iii. We should try to get a better quick release on the Lobos, we like the one on the flyer
2. Electrical

a. Cat’s meows not working needs to be tested-need to order more.
b. Check with Brett that email came through from Argos- emails did come
c. Batt voltage was 27V after completion, actual Batt voltage measured with the multimeter was 24V SO there is an offset with the voltage reading on the A/D.
3. Software

a. Why did we only get 7 pictures for 10 meter movement

i. Some images were not taken because the camera is not streaming the image and it times out while trying to grab a frame.

b. We will change the Transit image time stamps to start with sNtM, where N is the site number and M is the image number, then a date and time stamp will follow

c. Stack was put to sleep 10 times successfully but on the 11th it did not wake
i. Try test with spare bat3 board

d. We were having problems with the BAT3 before

e. No timeout errors on the motor controllers, we did increase the time out from 3 sec to 5 sec

f. Double check that the homing worked the first time
g. Still need to investigate whether our error recovery system was activated

