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I. Introduction

Coupling between a pelagically derived food supply and sediment community utilization of organic matter is critical to an understanding of biogeochemical cycling in the ocean [1, 2]. To resolve the coupling between pelagic and benthic systems, it is important to monitor the arrival and residence of organic matter on the sea floor using instrumentation capable of making measurements with appropriate spatial and temporal resolution. Critical questions which must be addressed to ultimately resolve pelagic-benthic coupling in the context of biogeochemical cycling are: 1) what is the quality and quantity of phytodetritus reaching the sea floor, and 2) what responses are elicited in the sediment community by the arrival of fresh detritus on the sea floor?

To address such critical questions, we began development of a new autonomous bottom-transecting instrument, the Rover, to make long time-series estimates of fresh phytodetritus arriving on the sea floor. The Rover will be capable of conducting non-invasive time-series measurements of phytopigment fluorescence as an indicator of fresh phytodetritus on the sediment surface. Sediment community metabolism measurements (e.g. sediment community oxygen consumption) will be conducted on the same sediments along transects including up to fifty sites without docking, recharging, or data download.

II. Mission Profile

The Rover is deployed by crane over the ship’s rail (Figure 1), and freefalls to the ocean bottom. After landing and waiting for disturbed sediment to settle, the Rover monitors the direction of the prevailing current and then moves up or cross current to avoid disturbance of measurement sites. The vehicle moves forward 10 meters, and waits for any disturbed sediments to settle down current away from the measurement site. While the Rover transits, a survey camera captures images of the surface sediment in the Rover’s path. After movement stops, two other cameras capture close-up optical images of the study site, and an imaging fluorometer, currently in development, will record the quantity and distribution of phytodetritus on the sediment. Next, two benthic respirometer chambers are inserted into the sediment one at a time. The chambers measure sediment community oxygen consumption (SCOC) for up to three days. After that time the chambers are raised and cleaned by water jets. The Rover then moves 10 m to a new study site and begins a new measurement cycle, repeating the sequence up to fifty times.

When the mission has been completed, commands are sent from a surface ship via acoustic modem, telling the Rover to release a 113 kg drop weight. The Rover then floats to the surface, where it is reattached to the ship’s crane and brought back on board.

The Rover is currently in the development phase and has been deployed on eighteen short test missions as of November 2008. The longest mission has been 16 days, but missions with fifty measurement sites may last greater than six months.

III. Vehicle Design

A. Mechanical Design

The mechanical configuration of the Rover is driven by two requirements: it must transit across very soft, sticky mud, and it must be capable of changing its buoyancy by 113 kg during each mission
.  In order to traverse the deep ocean mud, the Rover uses two 46 cm-wide, lugged tracks that present a 0.94 m2 footprint to support the Rover’s in-water weight of 68 kg. (Fig. 1 – Need a better image depicting all the parts of the Rover to help visualize the following description. The current Figure 1 just doesn’t do it) This low surface-contact pressure (72 kg/m2) allows the Rover to transit
 over the mud to minimize disturbance and suspended sediment.

Two brushless propulsion motors (model EC 60, Maxon Precision Motors, Fall River, Massachusetts) are mounted at the rear of the chassis. Each motor drives a 308:1 reduction gearhead and is contained in an oil-filled housing. The motors are rated at 400 watts each, but they consume less than 100 watts in this application. The gearhead output shafts are connected to the rear wheels via drive belts. 

The rover is 2.6 m long, 1.7 m wide, 1.5 m tall, and weighs 1136 kg in air. The vehicle frame is constructed of several 2.5 cm-thick black UHMW plates with grade 2 titanium pipes and brackets.  Most of the 0.54 m3 of 625 g/L syntactic foam is in the form of 13 blocks, each having a volume of 28 L and rated for 6000 m depth. Six more “football” floats on the upper titanium tubes provide additional flotation and can be adjusted fore and aft to trim the Rover’s pitch.

At the front of the Rover are two respirometer racks, which are lead-screw-driven vertical carriages that insert and extract the respirometer chambers. The two racks are completely independent to provide redundancy in case one system fails. 

The 113 kg steel drop weight is suspended below the Rover’s center of gravity using a series of lever-arms that are retained by a redundant pair of standard Benthos burn-wires. The Rover is ballasted to weigh 68 kg in water with the drop weight present, and to be 45 kg buoyant when the drop weight is released.

The 3 cm-diameter lift line for the Rover is attached to a titanium tube at the top of the vehicle between the two main bulkheads. To aid in recovery, the lift line is attached to a spar buoy with a 10 m-long polypropylene line. The spar buoy is a 6.5 m-long fiberglass and aluminum pole with a large football float in the middle and a steel weight at the bottom. The spar buoy holds a large flag, the VHF radio beacon, and the xenon flasher almost 3 m above the water, greatly enhancing the visibility of the Rover during recovery operations.

B. Instrumentation

Like most autonomous vehicles, the Rover platform exists to carry a suite of sensors. These instruments include:

• Benthic respirometers (2) 

• Respirometer chamber cameras (2) 

• Fluorometric cameras (2) 

• Survey camera

• Current meter

• Guest instruments (up to 3) 

Control and recovery of the Rover is aided by the following:

• Acoustic modem

• Argos satellite beacon

• VHF radio beacon

• Xenon flasher beacon

The most important measurement the Rover makes is of sediment community oxygen consumption. SCOC measurements are made by two respirometer chambers, each 30 cm in diameter and 20 cm deep (Figure 2). A titanium cutting edge on the bottom of each chamber reduces insertion forces and minimizes the adhesion of sticky sediment. Dissolved oxygen in the enclosed water of each chamber is measured by an optode (model 3830, Aanderaa Data Instruments, Bergen, Norway), with a third optode external to the chambers providing reference measurements of ambient water.

Each chamber has three valves on top that are opened during chamber insertion to avoid a bow wave and compression of the sediment to be studied, and again during extraction to avoid suction effects. The valves must remain tightly closed during respirometer incubations to minimize dissolved gas exchange with external water. Valves are hydraulically actuated with water pressure provided by a pump (model 5T, Sea-Bird Electronics, Bellevue, Washington) on each chamber, feeding the three valves in series. These custom hydraulic valves consume much less power than a solenoid-actuated valve, and their slow operation minimizes any pressure disturbances.

A pair of crossed rods, rotated at 6 rpm by a small motor during respirometer incubations, circulates the water inside each chamber. Stirring is required to avoid stratification of oxygen-depleted water while avoiding sediment resuspension.

After each respirometer measurement, the chamber is extracted from the sediment, and a cleaning pump sprays water across the interior surfaces of the chamber to remove adhering sediment that could affect subsequent measurements.

Two cameras (model Nova, Insite Pacific Inc., Solana Beach, California) mounted exterior to each chamber capture close-up images of the sediment inside the respirometers. These cameras have integral white LEDs to provide illumination. Images are captured before chamber insertion to record any visible fauna present on the sediment, and after chamber insertion to verify insertion depth and chamber sealing.

Prior to the placement of the respirometer chambers, two fluorometric scanners quantify the abundance, size, and distribution of phytodetritus on the sediment. Each scanner will scan a 30 cm by 35 cm patch of sediment directly beneath each respirometer chamber by moving a fluorometer (model ECO, WET Labs, Philomath, Oregon) back and forth across the study area in 1 mm steps, thus forming a fluorometric map of any phytodetritus present.

A 5 megapixel color survey camera (model GC2450, Prosilica Inc., Burnaby, B.C., Canada) captures images of the area in front of Rover about every meter while transiting between measurement sites. These images provide a continuous record of the area traversed by the Rover, and aid in surveys of phytodetritus, megafauna, and structural sediment features. [Brett to describe new strobe light] Two strobe lights (custom design, Scripps Institution of Oceanography, La Jolla, California) will provide illumination for the survey camera.
An acoustic current meter (model 2D-ACM, Falmouth Scientific, Inc., Cataumet, Massachusetts) measures current speed and direction for Rover navigation as well as a record of ambient conditions during deployment. The current meter also contains a compass and a tiltmeter so that the Rover’s heading, pitch, and roll can be determined.

The Rover can accommodate up to three guest instruments. The guest instrument ports supply switched power and an isolated RS-232 serial data connection. The power consumption and duty cycle of any guest instruments must be low enough to not adversely affect the energy remaining for other vehicle needs.

The Rover’s acoustic modem (model ATM-887, Benthos, North Falmouth, Massachusetts) is a data telemetry modem that has been modified by Benthos to provide a burn-wire output. The burn-wire is used to release the Rover’s recovery drop weight, and the data telemetry channel is used to send commands and receive status during a mission.

To aid in locating the Rover once it returns to the surface after a mission, it carries a VHF radio beacon (model RF700A1, Novatech, Dartmouth, Nova Scotia), a xenon flasher (model ST-400A, Novatech), and an Argos satellite beacon (model AS900A, Novatech).

C. Electrical Design

The main vehicle computer (MVC) is housed in a 43 cm-diameter cast titanium sphere rated to a depth of 6000 m. The MVC is a PC/104 board stack consisting of four cards: an ARM 9 computer card (model TS-7200, Technologic Systems, Fountain Hills, Arizona), a real-time clock daughter card (model TS-5620, Technologic Systems), a 12-port isolated serial card (model Xtreme/104 Isolated, Connect Tech, Inc., Guelph, Ontario), and a 5-port Ethernet switch (model PRV-1059, Parvus Corp., Salt Lake City, Utah). The TS-7200 was chosen mainly for its high performance-to-power-consumption ratio. The 200 MHz Cirrus ARM9 processor, 32 MB SDRAM, compact flash interface, and 10/100 Ethernet interface deliver more than adequate computational performance while consuming only 2 Watts during operation, and less than 0.5 Watts while idling. 

A network video server (model 241Q, Axis Communications, Lund, Sweden) captures images from the two chamber cameras and sends them via Ethernet to the MVC. The high-resolution survey camera is connected to the MVC via Ethernet directly. 

Also housed in the same sphere are electronics for power conversion and switching. Two off-the-shelf serially controlled 8-channel relay boards (model CK1610, Carl’s Electronics, Oakland, California) are used to switch power from the battery bus to all of the peripheral loads. This was a quick and inexpensive solution that enabled deployment and testing of the Rover; however, the cost of this short-term solution is wasted power, and no current, voltage, or ground-fault detection. Custom load controller boards are currently being designed that will have low quiescent power (a few mW), but are capable of providing up to hundreds of watts of galvanically isolated power at various voltages, and provide current and voltage monitoring, overcurrent protection, and ground fault detection. Until the load controllers are installed, the Rover has two DC-DC converters providing 5 VDC and 12 VDC (models UHE-5/5000-Q12 and UHE-12/2500–D24, Datel, Mansfield, Massachusetts) to loads that can’t operate directly from the 30 VDC bus.

All of the motors on the Rover, with the exception of the stirrer motors in the benthic respirometers, are brushless DC motors housed in oil. Attached to each oil-filled motor housing is a small 1-atm titanium pressure housing in which a motor driver/controller board (model EZSV23, All Motion, San Jose, California) is mounted. The motor controllers communicate with the MVC through an RS-485 multi-drop bus. The stirrer motors are brushed DC motors housed in Fluorinert. 

Rover power for short deployments is provided by alkaline battery packs that are housed in a single separate 43 cm-diameter titanium sphere. These alkaline packs consist of 240 D cells, with multiple diode-isolated strings of 20 cells providing a nominal 2.9 kW-h at 30 VDC. For future long-term deployments, two spheres of lithium primary batteries will provide up to 19 kW-h of energy.

D. Software Design

A simple operational scenario consisting of four serial phases drove the requirements for the Rover control system. After an initial launch phase, the Rover executes multiple movement and measurement phases to accumulate data at different measurement sites. When completed, the system enters the recovery phase where it waits for an acoustic command to ascend to the surface. The design of the control system directly reflects this scenario with classes designed to manage each phase. A supervisor process controls the transitions between phases. The code for the phase objects is designed to run as separate execution threads that are monitored by the control thread. Faults that occur during the execution of a phase are detected and trapped by the control thread, allowing the opportunity for recovery procedures to correct problems and perhaps continue with the mission.

The MVC runs a Linux 2.4-based operating system from Technologic Systems modified by MBARI to include the ConnectTech isolated serial card and the BusyBox command shell (www.busybox.net). The modular design of BusyBox resulted in a command shell tailored for use in the Rover and much smaller than a standard Linux shell environment.

The vehicle and instrument control applications are implemented in the Ruby programming language (www.ruby-lang.org). Ruby is a scripting language with many attributes of high-level languages that match-up well with rapid-development projects.

• Ruby is both object-oriented and dynamic, offering a high degree of flexibility

• The interpreter is implemented in C, reasonably fast, and portable to many embedded systems

• The concise syntax and powerful built-in features allow for quick application development and modifications

• The threading and exception capabilities improve error handling, isolation, and recovery

• Ruby applications are relatively simple and readable, making them more easily supported by non-programmers

• Ruby does not require a tool-chain for the target system – modifications can easily be made while field testing

The primary trade-off for these attributes is static, or compile-time, type-checking. Code compilation can greatly reduce run-time errors caused by using the wrong type of object in an expression. Since Ruby is a dynamic language, the type of object in any expression is not determined until run-time. This powerful feature precludes static variable type checking and can result in run-time errors that are normally caught in more traditional languages during compilation. The Rover team chose to address this issue primarily by extensive testing of all mission scenarios using software simulation and hybrid hardware-in-the-loop tests. The software simulations test all of the control system by using software interfaces to all of the physical vehicle devices. These tests can be “warped” to run much faster than real-time and in batch mode, providing a regression-test framework that can be run on a workstation. The hybrid tests run on the vehicle and exercise the entire deployed system using real device interfaces. However, these tests can also use the warping technique to jump over non-dynamic portions of the mission. This technique reduces hardware-in-the-loop testing time by 90 percent, allowing potential errors to be observed and corrected quickly.

IV. Deployments

E. Overview

Initial testing of the Rover’s ballast and trim was performed in MBARI’s 1.4 million liter saltwater test tank. The tank’s large size of 9 m width by 14 m length and 10 m depth provided enough volume to test the Rover’s drop weight release mechanism and the vehicle’s ability to move on the bottom.

The first at-sea testing took place from the R/V Pt. Lobos in Monterey Bay at a site about 40 km offshore and at a depth of 890 m, where the Rover was observed by the ROV Ventana. Subsequent dives at Station M, an abyssal area 220 km west of the central California coast, reached depths of over 4200 meters. These deep dives were launched from the R/V Atlantis and observed by the DSV Alvin. Later dives at Station M were launched from the R/V Western Flyer and observed with the ROV Tiburon.

The purpose of the first dives was to test launch and recovery mechanisms and procedures, and to verify basic Rover movement on the seafloor. After an acceptable level of mechanical reliability was established, the instruments were added and tested as well.

F. Propulsion System

Although the Rover was able to maneuver on the first dives, there were numerous issues with the track drive mechanism. The compensation oil reservoir levels for the main propulsion motors were greatly diminished after the first Rover dive. This is an important issue, as any loss of oil large enough to be observed during a short deployment could add up to a large and disabling loss during a long deployment. On the second dive, oil was observed escaping from the propulsion motor shaft seals. Rebuilding the motor output shafts and replacing the o-ring seals with lip seals has completely eliminated the oil loss problem.

While driving forward, the tracks were sometimes seen to stop briefly while the drive wheels continued to spin; this did not occur when driving in reverse. Further analysis revealed the cause of the problem. A track system with rear-wheel drive is in tension on the bottom half of the tracks and is loose on the top half while driving forward. This was causing the 1.5 cm-high treads on the tracks to interfere with parts of the chassis, such as protruding bolts and bulkheads. The problem was corrected by increasing the overall track tension slightly, and by installing smooth plastic sheets on the bottom of the chassis directly above the tracks. Knurling the surface of the drive wheels to increase contact friction with the tracks eliminated wheel slippage.

The tracks were observed to sit just on the sediment surface without sinking in, as was intended. However, sediment clinging to the track surface is carried forward on the top half of the tracks, acting as a conveyer belt, and dumped at the front of the vehicle near the respirometers. Stiff brushes added to the rear of the vehicle where the track leaves the seafloor have been effective in removing this sediment at the source.

Even with the brushes in place, simply moving too rapidly can kick up unacceptable quantities of sediment. In still water, Rover speeds above 2 cm/sec were found to be too disruptive. When the Rover is moving into a current, higher speeds are possible.  The vehicle chassis entrains some sediment-laden water during forward motion, and this water continues to move forward when the vehicle stops. If the ambient currents impinging on the front of the vehicle are too slow, then the disturbed sediment is deposited under the respirometer chambers, contaminating the study area. For this reason, the Rover’s speed should not exceed that of the ambient water currents.

Sediment disruption is not the only consideration when choosing the Rover’s speed. The Rover must move in the most energy-efficient manner to achieve the goal of operating in excess of six months on a single set of batteries. If the speed is too low, movement to a new site takes a long time and a lot of power is consumed by the “hotel load”, i.e. those loads such as the MVC, motor controllers, and cameras which are using power but are not contributing to the vehicle’s forward motion; only power consumed by the motors themselves does this. If the speed is too high, then hydrodynamic forces become large and power is wasted pushing through the water. Somewhere between these two extremes lies an optimum speed that minimizes total energy consumption.

To find this optimum speed, the Rover was operated in the test tank at various speeds while power consumption was monitored. These measurements are shown in Figure 5
, along with a least-squares fit of a curve of the form
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where Pt is the total power, Sr is the speed of the Rover, Ph is the hotel power, Cf is a constant that determines the power consumed by frictional forces in the drive mechanism, and Cw is a constant that determines the power consumed in pushing through the water. 

The total energy consumed by a Rover movement is then the power consumption during the move multiplied by the time required for the move, i.e. the distance divided by the speed


[image: image2.wmf]  

E

t

(

S

r

,

D

)

=

P

t

(

S

r

)

×

D

S

r






(2)

where Et is the total energy used for the move, and D is the distance traveled. Figure 4 shows the energy consumed as a function of Rover speed for three different distances with a hotel load of 30 W. The plots reveal that the least amount of energy is used under these conditions when the Rover moves at about 13.3 cm/s. It is also clear that for the range of speeds at which the Rover operates, the penalty for moving too slowly is much greater than that for moving too quickly. The minimum-energy speed doesn’t vary with distance traveled; moving twice the distance takes twice the energy, but the conditions that determine the optimum speed remain unchanged.

A different perspective can be gained by varying the hotel load instead of the distance traveled. Figure 5 shows the energy consumed for a 10 m move as a function of Rover speed for three different hotel loads. The minimum-energy speed decreases with a reduction in the hotel load, as the penalty for moving slowly is less severe. The minimum-energy speed also becomes more critical as the hotel load is reduced, although the effect is not a large one.

The Rover will likely be restricted to speeds below 10 cm/s to avoid the problem of disturbed sediment. It is in this regime that the greatest gains from a reduction in hotel load can be realized. The current hotel load, exceeding 30 W, will certainly be reduced in the future by installing the custom load controller boards and by decreasing the clock speed of the MVC. If the hotel load can be reduced to around 15 W, then the cost of a 10 m move at 5 cm/s can be reduced from 12 kJ to less than 9 kJ – a savings of 25 percent.

The power analysis thus far has followed that of traditional free-swimming AUVs [3,4]. The Rover, however, is different in one important aspect: it is not free-swimming and therefore its speed is restricted by conditions of the sediment and ambient bottom currents. Given that the Rover must always move against the current to carry away disturbed sediment, the energy cost of this current must be accounted for. Equation 1 can be modified to include a water current term that affects only the hydrodynamic forces
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where Sw is the speed of the water current. Figure 6 uses this new power equation to show the energy consumed for a 10 m move as a function of Rover speed in both still water and with a head current of 10 cm/s. As expected, moving into a current increases energy consumption at a given Rover speed. However, the current is not necessarily disadvantageous for the Rover’s energy consumption. In still water, the Rover is restricted to speeds of around 2 cm/s, at which about 20 kJ of energy are expended for a 10 m move. With a 10 cm/s current, the Rover can move at higher speeds without contaminating the study area. If, for instance, the Rover moves at 9 cm/s into a 10 cm/s head current, it expends around 15 kJ for the same 10 m move – a savings of 25 percent compared to a move with no current. Further gains may perhaps be realized by moving obliquely to the current, where most of the sediment-clearing effects of the current are retained without incurring the full hydrodynamic drag penalty.

G. Imaging System

[Describe here the chamber camera and survey camera results]

H. Benthic Respirometer Measurements

Only minor problems were encountered during testing of the respirometers. On one early dive, the switch that senses when the chamber is inserted to the correct depth into the sediment got stuck and did not activate. As a result, the chamber kept going until the rack limit switch was activated, and no damage was done. Had the rack limit switch failed, the motor controller overcurrent sensor would have tripped, protecting the motor and the rack. This was a good demonstration of the Rover’s layered structure, where systems are expected to eventually fail and other systems, hopefully seldom-used, activate to prevent disaster.

With the racks working, reliable respirometer measurements could be made. A typical SCOC measurement recorded at 890 m in Monterey Bay is shown in Figure 9. The reference optode shows more than 6 µM of variation in dissolved oxygen concentration over the 17 hours of the record. The chamber optode, however, shows a steady decrease in oxygen due to the respiration of organisms in the sediment. The slope of the chamber optode curve, which here is about -0.3 µM/hour, is an indicator of biological activity. SCOC measurements must be stopped before oxygen levels get prohibitively low, causing un-natural conditions.

One of the distinguishing features of the Rover is its ability to take duplicate respirometer incubations in multiple locations during a single deployment. Figure 10 shows the first three incubations taken during a deployment in Monterey Bay. The second and third show the expected negative linear slope characteristic, but the first incubation shows an initial increase in oxygen concentration. This is a known feature of these instruments, and is due to trapped air in the respirometer chamber. Although the chamber valves are opened soon after the Rover enters the water, it is impossible to release all of the air in the chambers. Small bubbles get trapped in the stirring motor assembly, and the acrylic chambers themselves may absorb some oxygen [5]. This excess oxygen is then released slowly into the chamber, affecting the first couple of incubations.

One strategy for dealing with this effect is to simply discard the first incubations, knowing that they don’t represent natural conditions. However, a closer examination of the first incubation can reveal some useful insights. Figure 11 shows the first curve of Figure 10 on an expanded scale. The change in oxygen concentration represented by these data points can be modeled by a curve of the form
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where O2 is the oxygen concentration, O2amb is the initial ambient oxygen concentration when the chamber is closed, O2bub is the total increase in oxygen concentration due to the trapped air, ( is the time constant for the release of the trapped oxygen, and K is the rate of decrease in oxygen concentration due to consumption by the sediment community. A least-squares fit of this curve to the data points yields the parameters shown in the figure.

These parameters indicate that the ambient oxygen concentration, O2amb, was 16.2 µM, and that the oxygen released from the trapped air would have caused an increase in concentration, O2bub, of 4.95 µM if no oxygen consumers were present. Knowing the value of O2bub enables us to calculate the volume of the bubble, at 1 atmosphere, that released this oxygen. Since the volume of the chamber inserted into the sediment is 9.0 L, we know that total amount of oxygen released is
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One mole of oxygen, or any gas, is 22.4 L at STP, but air is only 21 percent oxygen, so the size of the bubble at STP that would contain 45 µMoles of oxygen is
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Thus a relatively small volume of air trapped at the surface can have a large effect on the first measurements made at depth. [does this volume match that of the stirrer assembly void?]
The value of ( in Figure 11 suggests it takes 7.28 hours for 67 percent of the oxygen from the bubble to be released into the chamber. After three time constants, or about 22 hours, less than 5 percent of the oxygen in the bubble remains.

Finally, the value of K suggests that oxygen is being consumed at a rate that causes the concentration to fall by 0.327 µM/hour. This consumption rate could have been estimated by disregarding the first part of the curve and calculating the slope of only the last part, but by fitting the model to the whole measurement, more data are used and a more accurate result is obtained.

Note that the middle term in Equation 4 is empirically derived and may not represent the physics of the oxygen release mechanism. The actual rate of oxygen release is a complex function depending, among other things, on the surface area of the gas-water interface, which in turn depends on the unknown shape of the bubble or bubbles [6]. Some of the oxygen may be released from the acrylic chamber walls, which would have to be described in a different manner. In any case, the model is useful as it allows us to understand the quantities and time periods involved, and yields valid SCOC measurements from otherwise compromised data.

V. Conclusions and Future Work

Initial deployments of the Rover have been very successful. Thanks to the excellent vantage points provided by the ROVs Ventana and Tiburon, and DSV Alvin, numerous minor problems have been identified and addressed. 
An analysis of the Rover’s power use leads us to the somewhat surprising conclusion that energy can be saved by driving into a current. This knowledge will be incorporated into the vehicle software and will result in longer missions and more data. [What do we conclude about the imaging system?] Analysis of the respirometer chamber data shows that the Rover can make valid measurements of SCOC, and that the excess oxygen in the chambers can be accounted for by trapped air.

In the coming year the fluorometric imaging camera will be built and tested. The Rover will also be connected to the Monterey Accelerated Research System (MARS) cable for further testing in Monterey Bay (www.mbari.org/mars). The MARS cable will provide a continuous power and data connection to the Rover, which will greatly facilitate the development of the Rover’s autonomous software.
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Figures to be attached in separate file:

Figure 1 – Needs to show overall view of Rover. Is there a better pic?
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Figure 2 – Closeup of respirometer chambers
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Figure 3 – Power consumption vs speed graph
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Figure 4 – Energy consumption vs speed graph at different distances
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Figure 5 – Energy consumption vs speed graph at different hotel powers
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Figure 6 – Energy vs Speed with and without water current

[image: image12.png]Energy Used for 10 m Move

2y (k)

W, 5T

5 w0 15 E
Rover Speed (cms)




Figure 7 – Chamber image, before and after insertion

Figure 8 – Transect photomosaic

Figure 9 – Respirometer and reference optode
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Figure 10 – Three consecutive incubations
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Figure 11 – Curve fit to respirometer chamber with trapped air
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�Need to add depth capability here since it is critical to mechanical design.


�Float denotes positive buoyancy.


�Should not precede #4 – need to be reordered.
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