IODP – Monterey Bore Holes Functional/Design Requirements
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Functional Requirements                                  Design Requirements

Seismometer Borehole

Must Accommodate Drill string Re-Entry






Mud Skirt






Reentry Cone (removable)






4 DQ Landing Ring

Must Accommodate Wire Line Tool Entry






1~1.5 m entry cone (Rolled edges)

Must Accommodate Mars Secondary Node






Dim’s - ?

Must Accommodate ROVs and ROV Manipulators 






Access Doors ?






Removable Inst. Cages






48in ? x 48in ? platform






Maximum reach in (horizontal) = 






Maximum reach down (vertical) = 24in. ?

Must be Trawl Resistant

Hydrology Boreholes

Must Accommodate Drill string Re-Entry






Mud Skirt






Reentry Cone (removable)






3 DQ Landing Ring

Must Accommodate Wire Line Tool Entry






Pinned removable module

1~1.5 m entry cone (Rolled edges)

Must Accommodate Mars Secondary Node






Pinned removable module

Dim’s - ?

Must Accommodate ROVs and ROV Manipulators 






Access Doors ?






Removable Inst. Cages






48in ? x 48 in ? platform (Pinned removable module)






Plug Plate (Tubing Conn’s, Electrical Conn’s)






Maximum reach in (horizontal) = 






Maximum reach down (vertical) = 24in. ?

Must be Trawl Resistant

