MRS2 Test Dive – 4/13-4-15/10
Notes:   1) Quartz container traces are solid lines 
	2) All pumps were impeller type and started cycling at start-up and cycled on for 20 seconds every 2 minutes.
	3) QRD-2 broke a tie rod during the dive and was not used (~1/2 open during deployment)
	4) Batteries depleted to ~8.5 V approximately 37 hrs into deployment


























Results of note: 1) All three closed quartz chambers gave mostly useable traces although QRD-5 had an odd spike midway through the run.
		2) The open quartz chamber did not follow the ambient sensor as well as would be expected.
3) Three of the acrylic chambers produced unusable traces due to spiking (circulation issues?)
		4) Temperature traces were very tight w/ very little fluctuation in temperature during the dive. 
 
