“I just looked in the TT8 manual and it says it’s rated for 7 to 15 V input, so as long as we stay above 7 we’re ok. By the time the batt gets to 7 V / 3 = 2.3 V per cell they are *really* dead. I still don’t like the numbers but seeing that these values aren’t unusual for past deployments make me think it’s ok.” – PRM 4/23/18
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