While powering the camera with 7.60v from a wall power supply, these were the currents drawn for the following conditions:

1. sleep

40mA

2. start up

from 160-500mA for less than 10 s

3. taking a picture
up to 0.66A (ave about 0.33) for less 10 s 


Strobe circuit

We hooked up the strobe cable to gnd and a pull up resistor to 5v, when the camera fires the circuit is closed for 18 msec . The strobe signal is fired 80msec after the camera shutter signal is held low.
