1: SRVI battery pack:
6km working depth, 1.5 SF
87 lbs in air – with batteries
46 lbs in water - – with batteries
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2: SRVI camera housing
6km working depth, 1.5 SF
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Port seal:
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