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All actions assume 25V 5A external power and serial connection at 9600,8,N,1 through deck cable.
1. Test – choose Unit Tests from the main menu
a. Functions - Everything on the current controller menu
2. Pre-Deployment - choose Pre-deployment form from main menu
a. Set the current time
b. Image interval in minutes
c. Strobe charge time in seconds
d. Delay before starting deployment in minutes
e. Save options
3. Deployment - choose Deploy from main menu and remove external power
a. Delay for delay-time
b. Sleep for image-interval
c. Take image
i. Power on and charge strobes for maximum of charge-time seconds
ii. Power on and boot the cameras
iii. Trigger the camera shutters
iv. Power off cameras and strobes
d. Log before and after strobe voltages w/timestamp
e. Back to sleep for image-interval
4. Post-Deployment – return external power and choose Post-deployment form from main manu
a. Stop deployment
b. [bookmark: _GoBack]Request log data to be displayed
