Dualie Camera Tripod Specifications:
1. Far field imaged area: 20 m2
2. Near field imaged area: 2 m2
3. Strobe Energy: 2 x 200 Joules
4. Far field camera height:	 2.75 m	, angle: 30.5 deg
5. Near field camera height: 1.12m	, angle: 39 deg
6. Image frequency: 1 image/ hour
7. Object size resolutions of:
a. Bottom = 0.67 mm
b. Center = 0.96 mm
c. Top = 2.1 mm	
8. Weight:
9. Release mechanism: dual Benthos acoustic releases
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